

Ship Information

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| Ship Name: | La Touraine |
| Years in service: | 1891-1924 |
| Funnels: | 2 |
| Masts: | 3 |
| Shipping Line: | Compagnie Generale Transatlantique |
| Ship Description: | Built by Chantiers de Penhoet, St. Nazaire, France. Tonnage: 9,047. Dimensions: 520' x 56' (536' o.l.). Twin-screw, 19 knots. Triple expansion engines. Three masts and two funnels.  |
| History: | Launched, March 21, 1890. Maiden voyage: Havre-New York, June 20, 1891. At later date one mast was removed. Made a fast crossing from Havre to New York in 6 days, 18 hours. Made her final voyage to New York in 1922. Scrapped in France, 1924. |

 |